The performance greatly increased from PA4 to PA5. The bottleneck once again being the number of channels allowed as well as the request buffer size. Although with multiple event threads the performance actually slows down. The difference is created between the curves because the overhead of all the worker threads doesn’t exist anymore.